
**+ ADC Inputs or Analog PIN (A0, A1****, A2, A3, A4, A5):**

- Analog pin has 6 channels – PORTC0 to PORTC5 – with 10-bit resolution A/D convertor.

- These pins are connected to the analog header on the Arduino board.

**- It doesn’t only dedicated input for A/D function, But the reality is that you can use them as digital I/0.**